DS-2TD2836-25
Thermal & Optical Network Bullet Camera

						

	

Hikvision DS-2TD2836-25 Thermal Bi-spectrum Network Bullet Camera is applied to perimeter defense and fire-prevention purposes in critical infrastructures such as: airport, railway, prison, power station, 4S stores, and so on. The pre-alarm system helps you discover unexpected events immediately and protects you from property loss.
Smart Function (Thermal Imaging)
	Leading image processing technology: Adaptive AGC, DDE, 3D DNR, NETD less than 40 mk (@25°C,F#=1.0)
	Powerful behavior analysis function, based on deep learning algorithm: Line crossing, Intrusion, Region Entrance & Exit
	Reliable temperature exception alarm function
	Advanced fire detection algorithm
	Bi-spectrum image fusion, picture in picture preview
Thermal Imaging Module Function
	384 × 288 resolution sensor, high sensitivity sensor, support contrast adjustment
	Shutter adjustment in various modes
	3D DNR, 15 palettes of color adjustable, image detail enhancement
	Mirror image, digital zoom ×2, ×4, ×8, and local output

Specifications

Thermal Module	
Image Sensor	Vanadium Oxide Uncooled Focal Plane Arrays	
Max. Resolution	384 × 288	
Pixel Interval	17 μm	
Response Waveband	8 μm to 14 μm	
NETD	less than 40 mk (@25°C,F#=1.0)	
Lens (Focal Length)	25 mm	
MRAD	0.68 mrad	
Field of View	14.88°× 11.19° (H × V)	
Min. Focusing Distance	13 m	
Aperture	F 1.0	
Optical Module	
Max. Image Resolution	1920 × 1080	
Image Sensor	1/2.8” Progressive Scan CMOS	
Min. Illumination	Color: 0.001 Lux @(F1.2, AGC ON), B/W: 0.0001 Lux @(F1.2, AGC ON)	
Shutter Speed	1s to 1/100,000s	
Lens (Focal Length)	13 mm	
Field of View	24° × 13.7°(H × V)	
WDR	120 dB	
Day & Night	IR cut filter with auto switch	
Image Function	
Bi-spectrum Image Fusion	Fusion view of thermal view and overlaid details of the optical channel 	
Picture in Picture	Combins details of thermal and optical image PIP, overlay thermal image on optical image	
Smart Function	
VCA (Video Content Analysis)	4 VCA rule types (Line Crossing, Intrusion, Region Entrance, and Region Exiting), up to 8 VCA rules. 	
Temperature Measurement	3 temperature measurement rule types, 21 rules (10 points, 10 regions, and 1 line).	
Temperature Range	-20°C to +150°C (-4°F to +302°F)	
Temperature Accuracy	±8℃ (±14.4°F)	
Fire detection	Dynamic fire point detection, up to 10 fire points detectable.	
Infrared	
IR Distance	Up to 100 m	
IR Intensity and Angle	Automatically adjusted	
Network	
Main Stream	Visible Light: 50Hz: 25fps (1920 × 1080), 25fps (1280 × 960), 25fps (1280 × 720) 
Visible Light: 60Hz: 30fps (1920 × 1080), 30fps (1280 × 960), 30fps (1280 × 720)  
Thermal: 50fps ( 384 × 288)	
Sub Stream	Visible Light: 50Hz: 25fps (704 × 576), 25fps (352 × 288), 25fps (176 × 144) 
Visible Light: 60Hz: 30fps (704 × 480), 30fps (352 × 240), 30fps (176 × 120)  
Thermal: 50fps (384 × 288)	
Video Compression	H.265/H.264/MJPEG, H.265+/H.264+ encoding with Baseline/Main/High Profile	
Audio Compression	G .711u/G.711a/G.722.1/MP2L2/G.726/PCM	
Protocols	IPv4/IPv6, HTTP, HTTPS, 802.1x, Qos, FTP, SMTP, UPnP, SNMP, DNS, DDNS,NTP, RTSP, RTCP, RTP, TCP, UDP, IGMP, ICMP, DHCP, PPPoE	
Simultaneous Live View	Up to 20	
User/Host level	Up to 32 users, 3 levels: Administrator, Operator, User	
Security Measures	User authentication (ID and PW), MAC address binding, HTTPS encryption, IEEE 802.1x access control, IP address filtering	
Integration	
Alarm Input	2-ch inputs (0-5V DC)	
Alarm Output	2-ch relay outputs, alarm response actions configurable	
Alarm Action	SD recording/Relay output/Smart capture/FTP upload/Email linkage	
Audio Input	1 3.5mm Mic in/Line in interface. Line input: 2-2.4V[p-p], output impedance:1KΩ±10%	
Audio Output	Linear Level; Impedance: 600Ω	
Reset	1 Reset Button	
Ethernet	1 RJ45 10M/100M Self-adaptive Ethernet interface	
SD Memory Card	Built-in Micro SD card slot, support Micro SD/SDHC/SDXC card (up to 128G), support manual/alarm recording	
Analog Video Output	1.0V [p-p]/75Ω, PAL/NTSC/BNC	
Application Programming	Open-ended API, support ISAPI, HIKVISION SDK and third-party management platform	
Client	iVMS-4200	
Web Browser	IE9+, chrome31-chrome44, Firefox 30-Firefox51, Safari 5.02+(mac)	
General	
Menu language	English	
Power	24 VAC± 25%, 12 VDC± 20%, two-core terminal block  
PoE (802.3at, class 4)	
Power Consumption	24 VAC± 25%: 0.92 A, 12 VDC ± 20%: 1.9 A, max. 15W (22W with De-icing Heater On), PoE (802.3at, class 4): 42.5 V to 57 V, 0.4 A to 0.5 A	
Working Temperature/Humidity	-40 °C to 60 °C (-40 °F to 140 °F), 90% or less	
Protection Level	IP66 Standard 
TVS 6000V Lightning protection, surge protection, voltage transient protection	
Dimensions	535 mm × 171 mm × 400 mm (21.06 " × 6.73" × 15.75 ")	
Weight	Approx. 6 Kg (13.23 lb)	

Detection Range Table
* The table is only for reference, the performance may vary from camera to camera.
Smart functions Range
Different targets trigger the VCA events within different range limits.

VCA Range (Vehicles: 1.4×4.0m)	VCA Range (Humans: 1.8×0.5m)	Temperature Measurement (Object:2×2 m)	Temperature measurement (Object:1×1 m)	Fire Detection (Object:2×2 m)	Fire Detection (Object:1×1 m)	
750 m	250 m	585 m	295 m	1470 m	735 m	

Wide Range Coverage
There is range limit for detecting, recognizing, and identifying human/vehicle targets.

Detection Range (Vehicles: 1.4×4.0m)	Detection Range (Humans: 1.8×0.5m)	Recognition Range (Vehicles: 1.4×4.0m)	Recognition Range (Humans: 1.8×0.5m)	Identification Range (Vehicles: 1.4×4.0m)	Identification Range (Humans: 1.8×0.5m)	
2255 m	735 m	564 m	184 m	282 m	92 m	

Available Model
DS-2TD2836-25
Dimensions