DS-2TD2366-75
Thermal Network Bullet Camera

						

	

Hikvision DS-2TD2366-75 Thermal Network Bullet Camera is applied to perimeter defense and fire-prevention purposes in critical infrastructures such as: airport, railway, prison, power station, 4S stores, and so on. The pre-alarm system helps you discover unexpected events immediately and protects you from property loss.

Smart Function (Thermal Imaging)
	Leading image processing technology: Adaptive AGC, DDE, 3D DNR, NETD less than 40mk (@25°C,F#=1.0) 
	Powerful behavior analysis function, based on deep learning algorithm: Line crossing, Intrusion, Region Entrance & Exit
	Reliable temperature exception alarm function
	Advanced fire detection algorithm
Thermal Imaging Module Function
	640 × 512 resolution sensor, high sensitivity sensor, support contrast adjustment
	Shutter adjustment in various modes
	3D DNR, 15 palettes of color adjustable, image detail enhancement

Specifications

Thermal Module	
Image Sensor	Vanadium Oxide Uncooled Focal Plane Arrays	
Max. Resolution	640 × 512	
Pixel Interval	17 μm	
Response Waveband	8 μm to 14 μm	
NETD	less than 40mk (@25°C,F#=1.0) 	
Lens (Focal Length)	75 mm	
MRAD	0.23 mrad	
Field of View	8.3° × 6.64° (H × V)	
Min. Focusing Distance	8 m	
Aperture	F 1.0	
Smart Function	
VCA (Video Content Analysis)	4 VCA rule types (Line Crossing, Intrusion, Region Entrance, and Region Exiting), up to 8 VCA rules. 	
Temperature Measurement	3 temperature measurement rule types, 21 rules (10 points, 10 regions, and 1 line).	
Temperature Range	-20 °C to 150 °C (-4 °C to 302 °F) 	
Temperature Accuracy	± 8 °C (14.4 °F)	
Fire detection	Dynamic fire point detection, up to 10 fire points detectable.	
Network	
Main Stream	50fps (640×512, 384×288, 352×288)	
Sub Stream	50fps (640×512, 384×288, 352×288)	
Third Stream	50fps (640×512, 384×288, 352×288)	
Video Compression	H.265/H.264/MJPEG, H.265+/H.264+ encoding with Baseline/Main/High Profile	
Audio Compression	G .711u/G.711a/G.722.1/MP2L2/G.726/PCM	
Protocols	IPv4/IPv6, HTTP, HTTPS, 802.1x, Qos, FTP, SMTP, UPnP, SNMP, DNS, DDNS,NTP, RTSP, RTCP, RTP, TCP, UDP, IGMP, ICMP, DHCP, PPPoE, Bonjour	
Simultaneous Live View	Up to 20	
User/Host level	Up to 32 users, 3 levels: Administrator, Operator, User	
Security Measures	User authentication (ID and PW), MAC address binding, HTTPS encryption, IEEE 802.1x access control, IP address filtering	
Integration	
Alarm Input	2-ch inputs (0-5V DC)	
Alarm Output	2-ch relay outputs, alarm response actions configurable	
Alarm Action	Preset/Patrol Scan/Pattern Scan/SD Card Record/Relay Output/Smart capture/FTP upload/Email linkage	
Audio Input	1 3.5mm Mic in/Line in interface. Line input: 2-2.4V[p-p], output impedance:1KΩ±10%	
Audio Output	Linear Level; Impedance: 600Ω	
Ethernet	1 RJ45 10M/100M Self-adaptive Ethernet interface	
SD Memory Card	Built-in Micro SD card slot, support Micro SD/SDHC/SDXC card (up to 64G), support manual/alarm recording	
Analog Video Output	1.0V [p-p]/75Ω, PAL/NTSC/BNC	
Application Programming	Open-ended API, support ISAPI, HIKVISION SDK and third-party management platform	
Client	iVMS-4200	
Web Browser	IE9+, chrome31-chrome44, Firefox 30-Firefox51, Safari 5.02+(mac)	
General	
Menu language	English	
Power	24 VAC± 25%, 12 VDC± 20%, two-core terminal block 	
Power Consumption	24 VAC± 25%: 0.92 A, 12 VDC ± 20%: 1.9 A, max. 8W (22W with De-icing Heater On)	
Working Temperature/Humidity	-40 °C to 65 °C (-40 °F to 149 °F), 90% or less	
Protection Level	IP66 Standard 
TVS 6000V Lightning protection, surge protection, voltage transient protection	
Dimensions	535mm × 400mm × 171mm (21.06" × 15.75" × 6.73") 	
Weight	 Approx. 6.40 kg (14.11 lb)	

Detection Range Table
* The table is only for reference, the performance may vary from camera to camera.
Smart functions Range
Different targets trigger the VCA events within different range limits.

VCA Range (Vehicles: 1.4×4.0m)	VCA Range (Humans: 1.8×0.5m)	Temperature Measurement (Object:2×2 m)	Temperature measurement (Object:1×1 m)	Fire Detection (Object:2×2 m)	Fire Detection (Object:1×1 m)	
2250 m	750 m	1775 m	885 m	4410 m	2205 m	

Wide Range Coverage
There is range limit for detecting, recognizing, and identifying human/vehicle targets.

Detection Range (Vehicles: 1.4×4.0m)	Detection Range (Humans: 1.8×0.5m)	Recognition Range (Vehicles: 1.4×4.0m)	Recognition Range (Humans: 1.8×0.5m)	Identification Range (Vehicles: 1.4×4.0m)	Identification Range (Humans: 1.8×0.5m)	
6765 m	2206 m	1691 m	551 m	846 m	276 m	

Available Model
DS-2TD2366-75
Dimensions